#
# Example of the new header for an RMG type file
#
#   In this example, several parameters are specified, even though
#   they have the default value and could be omitted.  Note that 
#   parameters without a set name precedding them apply to all the 
#   data sets in the file.
#

set_name           (&)       = RCS  DTE
set_rows           (pixels)  =   1250
set_cols           (pixels)  =   1250
set_hddr           (bytes)   =      0
set_tail           (bytes)   =      0
set_proj           (&)       = sch
set_plat           (deg)     =     34.10324
set_plon           (deg)     =   -123.63922
set_phdg           (deg)     =    180.00000

row_mult           (m)       =      5.00000
row_addr           (m)       =      0.00000

col_mult           (m)       =      5.00000
col_addr           (m)       =      0.00000

val_size           (bytes)   =      4
val_frmt           (&)       = REAL*4
val_endi           (&)       = BIG ENDIAN

rcs.row_hddr       (bytes)   =      0
rcs.row_tail       (bytes)   =   5000
rcs.col_hddr       (bytes)   =      0
rcs.col_tail       (bytes)   =      0
rcs.val_mult       (-)       =      1.0
rcs.val_addr       (-)       =      0.0
rcs.val_minv       (dB)      =      0.1
rcs.val_maxv       (dB)      =     10.0
rcs.val_null       (-)       =  

dte.row_hddr       (bytes)   =   5000
dte.row_tail       (bytes)   =      0
dte.col_hddr       (bytes)   =      0
dte.col_tail       (bytes)   =      0
dte.val_mult       (m)       =      1.0
dte.val_addr       (m)       =      0.0
dte.val_minv       (m)       =     10.0
dte.val_maxv       (m)       =  10000.0
dte.val_null       (m)       =  
